Main Mounting Plate
· Enable supports, on build plate only
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Primary Battery Mount:
· Print in upright position so that layer lines won’t separate on bolt through holes due to battery weight.
· Enable supports 
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Top Shell
· Print rotated -60 degrees in the x direction
· Enable supports with these settings: type: tree (auto), style: tree strong. Top Interface Layers: 3. Top Interface Spacing: 0.08 mm. Support/object xy distance: 0.15. Branch Distance: 3mm. Branch Angle: 35 degrees/
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Bottom Shell
· No supports required
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Handle Base
· Rotate 110 degrees in the x direction
· 100% infill (rectilinear)
· Enable supports, type:tree, style:Tree Strong, on build plate only checked (true), remove small overhangs unchecked (false)
· Top interface layers:3, Top interface spacing:0.08mm, Support/object xy distance: 0.15 mm, Branch Distance: 3mm, Branch Angle: 35 
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